# [Mailbox Configuration Wizard] - [Scanner Specification]

When you display this screen for the first time, multifunction devices on the same subnet as the PC and accessible to the mailbox are filtered, and then [Searched Scanner] shows the result.
Select one from the [Searched Scanner] list and click [Next].
When connecting to a multifunction device on a different subnet from the PC, enter the multifunction machine IP address or FQDN in [Specify the IP address or FQDN directly], and then click [Next].

### [Specify the IP address or FQDN directly]

Enter the multifunction device IP address or FQDN to connect. Up to 255 characters can be entered.
You can enter either IPv4 or IPv6 address.

### [Searched Scanner]

After filtering, [Searched Scanner] shows the multifunction devices that are on the same subnet as the PC and accessible to the mailbox.
Select one from the list, and click [Next].

#### [Name]

Displays the name of the multifunction device.

#### [Device Name]

Displays the model name of the multifunction device.

#### [IP Address / FQDN]

Displays the IP address of the multifunction device.

#### [Location]

Displays the location of the multifunction device.

### [Repeat Search]

Re-retrieves the multifunction device on the same subnet as the PC.

### [Search Settings]

When you want to search a multifunction device using the SNMP community name, click this. The [Search Settings] dialog box appears. Using this dialog box, specify the SNMP community name (read-only) of the multifunction device.

### [Back]

Displays the [Mailbox Configuration] screen.

### [Next]

Displays the [Mailbox Specification] screen.